What:           /sys/kernel/debug/hyperv/<UUID>/fuzz_test_state
Date:           October 2019
KernelVersion:  5.5
Contact:        Branden Bonaby <brandonbonaby94@gmail.com>
Description:    Fuzz testing status of a vmbus device, whether its in an ON
                state or a OFF state
Users:          Debugging tools

What:           /sys/kernel/debug/hyperv/<UUID>/delay/fuzz_test_buffer_interrupt_delay
Date:           October 2019
KernelVersion:  5.5
Contact:        Branden Bonaby <brandonbonaby94@gmail.com>
Description:    Fuzz testing buffer interrupt delay value between 0 - 1000
		 microseconds (inclusive).
Users:          Debugging tools

What:           /sys/kernel/debug/hyperv/<UUID>/delay/fuzz_test_message_delay
Date:           October 2019
KernelVersion:  5.5
Contact:        Branden Bonaby <brandonbonaby94@gmail.com>
Description:    Fuzz testing message delay value between 0 - 1000 microseconds
		 (inclusive).
Users:          Debugging tools
