What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage0-1_i_calibphase
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write unscaled value for the Local Oscillatior path quadrature I phase shift.

What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage0-1_q_calibphase
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write unscaled value for the Local Oscillatior path quadrature Q phase shift.

What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage0_i_calibbias
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write value for the Local Oscillatior Feedthrough Offset Calibration I Positive
		side.

What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage0_q_calibbias
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write value for the Local Oscillatior Feedthrough Offset Calibration Q Positive side.

What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage1_i_calibbias
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write raw value for the Local Oscillatior Feedthrough Offset Calibration I Negative
		side.

What:		/sys/bus/iio/devices/iio:deviceX/in_altvoltage1_q_calibbias
KernelVersion:
Contact:	linux-iio@vger.kernel.org
Description:
		Read/write raw value for the Local Oscillatior Feedthrough Offset Calibration Q Negative
		side.
