What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_dither_enable
KernelVersion:	5.12
Contact:	linux-iio@vger.kernel.org
Description:
		Dither enable. Write 1 to enable dither or 0 to disable it.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_dither_invert
KernelVersion:	5.12
Contact:	linux-iio@vger.kernel.org
Description:
		Inverts the dither applied to the selected DAC channel. Dither is not
		inverted by default. Write "1" to invert dither.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_dither_scale_available
KernelVersion:	5.12
Contact:	linux-iio@vger.kernel.org
Description:
		Returns possible scalings available for the current channel.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_dither_scale
KernelVersion:	5.12
Contact:	linux-iio@vger.kernel.org
Description:
		Scales the dither before it is applied to the selected channel.

What:		/sys/bus/iio/devices/iio:deviceX/in_voltageY_dither_source
KernelVersion:	5.12
Contact:	linux-iio@vger.kernel.org
Description:
		Selects dither source applied to the selected channel. Write "0" to
		select N0 source, write "1" to select N1 source.
